**PWS-870 Embedded Controller FW flashing**

|  |  |  |  |
| --- | --- | --- | --- |
| **Data Create** | 2014/11/06 | **Release Note** | □ Internal ■ External |
| **Category** | FAQ | **Product Group** | SAG |
| **Function** | EC FW update | **Related OS** | - |
| **Related Product** | PWS-870 | | |

**[Abstract]**


PWS-870 may have an issue that there are a few seconds of non-reactive time when device wake up from sleep or hibernation. Updating the EC FW can fix this problem

**[Preparation]**

1. 
2. DOS bootable media
3. The .bin file to flash, name it **EC.bin**

**[Solution]**

Unzip the attached file (**EC\_FW\_flashing.zip**) above.



Copy the file **clear.EXE**, **IFU.EXE** and **EC.bin** to the DOS bootable media, and then boot your device under DOS.

|  |
| --- |
| **C:\>dir**  **Volume in drive C is ABC**  **Volume Serial Number id XXXX-XXXX**  **Directory of C:\**  **CLEAR EXE 10,056 03-10-14 4:47p**  **IFU EXE 17,750 04-14-10 3:09p**  **EC BIN 98,304 11-06-14 3:44p** |

Execute **clear**, and click **Enter**.

|  |
| --- |
| **C:\>clear**  **eeprom table erase successful.** |

Execute **ifu EC.bin**, and click **Enter**.

|  |
| --- |
| **C:\>ifu EC.bin** |

The device will update the EC FW and turn off. Now unplug the power input. Plug the power input and boot. The EC FW is successfully updated.